TEST REPORT
SUMMARY

Description                "scenario_vlan" result report
Start Time                  2026-09-22T18:55:31.107542
	Index
	Scenario
	Time Stamp
	Pass/Fail

	1
	Print Topology Image
	18:56:20
	1 / 0

	2
	Session Check
	18:56:20
	6 / 0

	3
	Check SONiC OS Version
	18:56:20
	2 / 0

	4
	Create Vlan
	18:56:31
	10 / 0

	5
	Add Vlan Member
	18:57:27
	10 / 0

	6
	Assign IP Address to Host
	18:58:23
	8 / 0

	7
	Test Network-link
	18:58:23
	2 / 0

	8
	Delete IP Address to Host
	18:58:32
	8 / 0



SESSIONS

	Name
	Connection Type
	Host Address
	Port
	Login User

	H-1
	ssh
	10.250.0.101
	22
	ubuntu

	H-2
	ssh
	10.250.0.102
	22
	ubuntu

	H-3
	ssh
	10.250.0.103
	22
	ubuntu

	H-4
	ssh
	10.250.0.104
	22
	ubuntu

	SW-1
	ssh
	10.250.0.10
	22
	admin

	SW-2
	ssh
	10.250.0.11
	22
	admin



RESULT

	Index
	Action
	Session
	Time Stamp
	Pass/Fail

	1
	print topo img
	caller
	18:56:20
	Pass

	Parameter
	topo-L2-Vlan.jpg

	Response
	[image: ]

	

	2
	session check SW-1
	SW-1
	18:56:20
	Pass

	Parameter
	None

	Response
	Linux SW-1 6.1.0-29-2-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.1.123-1 (2025-01-02) x86_64
You are on
  ____   ___  _   _ _  ____
 / ___| / _ \| \ | (_)/ ___|
 \___ \| | | |  \| | | |
  ___) | |_| | |\  | | |___
 |____/ \___/|_| \_|_|\____|

-- Software for Open Networking in the Cloud --

Unauthorized access and/or use are prohibited.
All access and/or use are subject to monitoring.

Help:    https://sonic-net.github.io/SONiC/

Last login: Tue Sep 22 18:48:00 2026 from 10.250.0.1

admin@SW-1:~$ 

	3
	session check SW-2
	SW-2
	18:56:20
	Pass

	Parameter
	None

	Response
	Linux SW-2 6.1.0-29-2-amd64 #1 SMP PREEMPT_DYNAMIC Debian 6.1.123-1 (2025-01-02) x86_64
You are on
  ____   ___  _   _ _  ____
 / ___| / _ \| \ | (_)/ ___|
 \___ \| | | |  \| | | |
  ___) | |_| | |\  | | |___
 |____/ \___/|_| \_|_|\____|

-- Software for Open Networking in the Cloud --

Unauthorized access and/or use are prohibited.
All access and/or use are subject to monitoring.

Help:    https://sonic-net.github.io/SONiC/

Last login: Tue Sep 22 18:48:02 2026 from 10.250.0.1

admin@SW-2:~$ 

	4
	session check H-1
	H-1
	18:56:20
	Pass

	Parameter
	None

	Response
	Welcome to Ubuntu 20.04.6 LTS (GNU/Linux 5.4.0-215-generic x86_64)

 * Documentation:  https://help.ubuntu.com
 * Management:     https://landscape.canonical.com
 * Support:        https://ubuntu.com/pro

 System information as of Tue Sep 22 09:56:06 UTC 2026

  System load:  0.04              Processes:             145
  Usage of /:   9.0% of 19.20GB   Users logged in:       0
  Memory usage: 6%                IPv4 address for Eth1: 10.0.100.10
  Swap usage:   0%


Expanded Security Maintenance for Applications is not enabled.

0 updates can be applied immediately.

Enable ESM Apps to receive additional future security updates.
See https://ubuntu.com/esm or run: sudo pro status


The list of available updates is more than a week old.
To check for new updates run: sudo apt update
New release '22.04.5 LTS' available.
Run 'do-release-upgrade' to upgrade to it.


*** System restart required ***
Last login: Tue Sep 22 09:48:05 2026 from 10.250.0.1

ubuntu@H-1:~$ 

	5
	session check H-2
	H-2
	18:56:20
	Pass

	Parameter
	None

	Response
	Welcome to Ubuntu 20.04.6 LTS (GNU/Linux 5.4.0-215-generic x86_64)

 * Documentation:  https://help.ubuntu.com
 * Management:     https://landscape.canonical.com
 * Support:        https://ubuntu.com/pro

 System information as of Tue Sep 22 09:56:08 UTC 2026

  System load:  0.04              Processes:             140
  Usage of /:   9.0% of 19.20GB   Users logged in:       0
  Memory usage: 6%                IPv4 address for Eth1: 10.0.100.11
  Swap usage:   0%


Expanded Security Maintenance for Applications is not enabled.

0 updates can be applied immediately.

Enable ESM Apps to receive additional future security updates.
See https://ubuntu.com/esm or run: sudo pro status


The list of available updates is more than a week old.
To check for new updates run: sudo apt update
New release '22.04.5 LTS' available.
Run 'do-release-upgrade' to upgrade to it.


*** System restart required ***
Last login: Tue Sep 22 09:48:07 2026 from 10.250.0.1

ubuntu@H-2:~$ 

	6
	session check H-3
	H-3
	18:56:20
	Pass

	Parameter
	None

	Response
	Welcome to Ubuntu 20.04.6 LTS (GNU/Linux 5.4.0-215-generic x86_64)

 * Documentation:  https://help.ubuntu.com
 * Management:     https://landscape.canonical.com
 * Support:        https://ubuntu.com/pro

 System information as of Tue Sep 22 09:56:10 UTC 2026

  System load:  0.0               Processes:             144
  Usage of /:   9.0% of 19.20GB   Users logged in:       0
  Memory usage: 6%                IPv4 address for Eth1: 10.0.100.12
  Swap usage:   0%                IPv4 address for Eth1: 10.0.200.10


Expanded Security Maintenance for Applications is not enabled.

0 updates can be applied immediately.

Enable ESM Apps to receive additional future security updates.
See https://ubuntu.com/esm or run: sudo pro status


The list of available updates is more than a week old.
To check for new updates run: sudo apt update
New release '22.04.5 LTS' available.
Run 'do-release-upgrade' to upgrade to it.


*** System restart required ***
Last login: Tue Sep 22 09:48:09 2026 from 10.250.0.1

ubuntu@H-3:~$ 

	7
	session check H-4
	H-4
	18:56:20
	Pass

	Parameter
	None

	Response
	Welcome to Ubuntu 20.04.6 LTS (GNU/Linux 5.4.0-215-generic x86_64)

 * Documentation:  https://help.ubuntu.com
 * Management:     https://landscape.canonical.com
 * Support:        https://ubuntu.com/pro

 System information as of Tue Sep 22 09:56:12 UTC 2026

  System load:  0.0               Processes:             144
  Usage of /:   9.0% of 19.20GB   Users logged in:       0
  Memory usage: 6%                IPv4 address for Eth1: 10.0.100.13
  Swap usage:   0%                IPv4 address for Eth1: 10.0.200.11


Expanded Security Maintenance for Applications is not enabled.

0 updates can be applied immediately.

Enable ESM Apps to receive additional future security updates.
See https://ubuntu.com/esm or run: sudo pro status


The list of available updates is more than a week old.
To check for new updates run: sudo apt update
New release '22.04.5 LTS' available.
Run 'do-release-upgrade' to upgrade to it.


*** System restart required ***
Last login: Tue Sep 22 09:48:12 2026 from 10.250.0.1

ubuntu@H-4:~$ 

	

	8
	Check SONiC OS Version
	SW-1
	18:56:20
	Pass

	Parameter
	~$ show version

	Response
	
SONiC Software Version: SONiC.202505.926279-b7206d85a
SONiC OS Version: 12
Distribution: Debian 12.11
Kernel: 6.1.0-29-2-amd64
Build commit: b7206d85a
Build date: Tue Aug 19 14:16:31 UTC 2025
Built by: azureuser@d674752fc000000

Platform: x86_64-kvm_x86_64-r0
HwSKU: Etri-SONiC
ASIC: vs
ASIC Count: 1
Serial Number: N/A
Model Number: N/A
Hardware Revision: N/A
Uptime: 18:56:20 up 26 min,  1 user,  load average: 0.61, 1.28, 1.07
Date: Tue 22 Sep 2026 18:56:20

Docker images:
REPOSITORY                    TAG                       IMAGE ID       SIZE
docker-macsec                 202505.926279-b7206d85a   eb3fac1f1e14   347MB
docker-macsec                 latest                    eb3fac1f1e14   347MB
docker-orchagent              202505.926279-b7206d85a   1d3a6e9b7605   356MB
docker-orchagent              latest                    1d3a6e9b7605   356MB
docker-sflow                  202505.926279-b7206d85a   f7c21d48ff02   345MB
docker-sflow                  latest                    f7c21d48ff02   345MB
docker-teamd                  202505.926279-b7206d85a   219394382f06   344MB
docker-teamd                  latest                    219394382f06   344MB
docker-fpm-frr                202505.926279-b7206d85a   231b5d766152   393MB
docker-fpm-frr                latest                    231b5d766152   393MB
docker-nat                    202505.926279-b7206d85a   553569c2ed1a   347MB
docker-nat                    latest                    553569c2ed1a   347MB
docker-dash-ha                202505.926279-b7206d85a   eadcbe8a318f   357MB
docker-dash-ha                latest                    eadcbe8a318f   357MB
docker-syncd-vs               202505.926279-b7206d85a   d6f77d7d5c73   2.18GB
docker-syncd-vs               latest                    d6f77d7d5c73   2.18GB
docker-gbsyncd-vs             202505.926279-b7206d85a   e1b2e95f057b   2.18GB
docker-gbsyncd-vs             latest                    e1b2e95f057b   2.18GB
docker-sonic-bmp              202505.926279-b7206d85a   773e76990a92   315MB
docker-sonic-bmp              latest                    773e76990a92   315MB
docker-dhcp-relay             202505.926279-b7206d85a   b82ba73b313a   323MB
docker-dhcp-relay             latest                    b82ba73b313a   323MB
docker-platform-monitor       202505.926279-b7206d85a   dff6c6e2ea25   447MB
docker-platform-monitor       latest                    dff6c6e2ea25   447MB
docker-snmp                   202505.926279-b7206d85a   f813952ac4d7   358MB
docker-snmp                   latest                    f813952ac4d7   358MB
docker-router-advertiser      202505.926279-b7206d85a   e8cbc5b10fff   314MB
docker-router-advertiser      latest                    e8cbc5b10fff   314MB
docker-mux                    202505.926279-b7206d85a   a6ccc3ca8b81   366MB
docker-mux                    latest                    a6ccc3ca8b81   366MB
docker-gnmi-watchdog          202505.926279-b7206d85a   9871849025e5   314MB
docker-gnmi-watchdog          latest                    9871849025e5   314MB
docker-lldp                   202505.926279-b7206d85a   ee7a4d514875   360MB
docker-lldp                   latest                    ee7a4d514875   360MB
docker-sonic-gnmi             202505.926279-b7206d85a   9f8ed5aefa5d   427MB
docker-sonic-gnmi             latest                    9f8ed5aefa5d   427MB
docker-bmp-watchdog           202505.926279-b7206d85a   62eb09ee3d7e   314MB
docker-bmp-watchdog           latest                    62eb09ee3d7e   314MB
docker-eventd                 202505.926279-b7206d85a   b5707e85d1ec   314MB
docker-eventd                 latest                    b5707e85d1ec   314MB
docker-database               202505.926279-b7206d85a   6d85154e4f52   321MB
docker-database               latest                    6d85154e4f52   321MB
docker-auditd-watchdog        202505.926279-b7206d85a   92489e94897e   314MB
docker-auditd-watchdog        latest                    92489e94897e   314MB
docker-auditd                 202505.926279-b7206d85a   5e7f418566b0   314MB
docker-auditd                 latest                    5e7f418566b0   314MB
docker-dash-engine            202505.926279-b7206d85a   9b719283bb99   697MB
docker-dash-engine            latest                    9b719283bb99   697MB
docker-sonic-mgmt-framework   202505.926279-b7206d85a   347d1879e56e   403MB
docker-sonic-mgmt-framework   latest                    347d1879e56e   403MB
docker-sysmgr                 202505.926279-b7206d85a   acdc8191fd32   326MB
docker-sysmgr                 latest                    acdc8191fd32   326MB


	Judgement
	Success

inter-conditional operator    :   or
contain string:    SONiC OS Version: 12
contain string:    SONiC Software Version: SONiC.master.775830-a7eb965c8
not contain string:    Error:

	9
	Check SONiC OS Version
	SW-2
	18:56:25
	Pass

	Parameter
	~$ show version

	Response
	
SONiC Software Version: SONiC.202505.926279-b7206d85a
SONiC OS Version: 12
Distribution: Debian 12.11
Kernel: 6.1.0-29-2-amd64
Build commit: b7206d85a
Build date: Tue Aug 19 14:16:31 UTC 2025
Built by: azureuser@d674752fc000000

Platform: x86_64-kvm_x86_64-r0
HwSKU: Etri-SONiC
ASIC: vs
ASIC Count: 1
Serial Number: N/A
Model Number: N/A
Hardware Revision: N/A
Uptime: 18:56:25 up 26 min,  1 user,  load average: 1.50, 1.63, 1.19
Date: Tue 22 Sep 2026 18:56:25

Docker images:
REPOSITORY                    TAG                       IMAGE ID       SIZE
docker-macsec                 202505.926279-b7206d85a   eb3fac1f1e14   347MB
docker-macsec                 latest                    eb3fac1f1e14   347MB
docker-orchagent              202505.926279-b7206d85a   1d3a6e9b7605   356MB
docker-orchagent              latest                    1d3a6e9b7605   356MB
docker-sflow                  202505.926279-b7206d85a   f7c21d48ff02   345MB
docker-sflow                  latest                    f7c21d48ff02   345MB
docker-teamd                  202505.926279-b7206d85a   219394382f06   344MB
docker-teamd                  latest                    219394382f06   344MB
docker-fpm-frr                202505.926279-b7206d85a   231b5d766152   393MB
docker-fpm-frr                latest                    231b5d766152   393MB
docker-nat                    202505.926279-b7206d85a   553569c2ed1a   347MB
docker-nat                    latest                    553569c2ed1a   347MB
docker-dash-ha                202505.926279-b7206d85a   eadcbe8a318f   357MB
docker-dash-ha                latest                    eadcbe8a318f   357MB
docker-gbsyncd-vs             202505.926279-b7206d85a   e1b2e95f057b   2.18GB
docker-gbsyncd-vs             latest                    e1b2e95f057b   2.18GB
docker-syncd-vs               202505.926279-b7206d85a   d6f77d7d5c73   2.18GB
docker-syncd-vs               latest                    d6f77d7d5c73   2.18GB
docker-sonic-bmp              202505.926279-b7206d85a   773e76990a92   315MB
docker-sonic-bmp              latest                    773e76990a92   315MB
docker-dhcp-relay             202505.926279-b7206d85a   b82ba73b313a   323MB
docker-dhcp-relay             latest                    b82ba73b313a   323MB
docker-platform-monitor       202505.926279-b7206d85a   dff6c6e2ea25   447MB
docker-platform-monitor       latest                    dff6c6e2ea25   447MB
docker-snmp                   202505.926279-b7206d85a   f813952ac4d7   358MB
docker-snmp                   latest                    f813952ac4d7   358MB
docker-router-advertiser      202505.926279-b7206d85a   e8cbc5b10fff   314MB
docker-router-advertiser      latest                    e8cbc5b10fff   314MB
docker-mux                    202505.926279-b7206d85a   a6ccc3ca8b81   366MB
docker-mux                    latest                    a6ccc3ca8b81   366MB
docker-gnmi-watchdog          202505.926279-b7206d85a   9871849025e5   314MB
docker-gnmi-watchdog          latest                    9871849025e5   314MB
docker-lldp                   202505.926279-b7206d85a   ee7a4d514875   360MB
docker-lldp                   latest                    ee7a4d514875   360MB
docker-sonic-gnmi             202505.926279-b7206d85a   9f8ed5aefa5d   427MB
docker-sonic-gnmi             latest                    9f8ed5aefa5d   427MB
docker-bmp-watchdog           202505.926279-b7206d85a   62eb09ee3d7e   314MB
docker-bmp-watchdog           latest                    62eb09ee3d7e   314MB
docker-eventd                 202505.926279-b7206d85a   b5707e85d1ec   314MB
docker-eventd                 latest                    b5707e85d1ec   314MB
docker-database               202505.926279-b7206d85a   6d85154e4f52   321MB
docker-database               latest                    6d85154e4f52   321MB
docker-auditd-watchdog        202505.926279-b7206d85a   92489e94897e   314MB
docker-auditd-watchdog        latest                    92489e94897e   314MB
docker-auditd                 202505.926279-b7206d85a   5e7f418566b0   314MB
docker-auditd                 latest                    5e7f418566b0   314MB
docker-dash-engine            202505.926279-b7206d85a   9b719283bb99   697MB
docker-dash-engine            latest                    9b719283bb99   697MB
docker-sonic-mgmt-framework   202505.926279-b7206d85a   347d1879e56e   403MB
docker-sonic-mgmt-framework   latest                    347d1879e56e   403MB
docker-sysmgr                 202505.926279-b7206d85a   acdc8191fd32   326MB
docker-sysmgr                 latest                    acdc8191fd32   326MB


	Judgement
	Success

inter-conditional operator    :   or
contain string:    SONiC OS Version: 12
contain string:    SONiC Software Version: SONiC.master.775830-a7eb965c8
not contain string:    Error:

	

	10
	Check VLAN exist on SW-1
	SW-1
	18:56:31
	Pass

	Parameter
	~$ show vlan config

	Response
	Name    VID    Member    Mode
------  -----  --------  ------


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    Error:

	11
	Check VLAN exist on SW-2
	SW-2
	18:56:37
	Pass

	Parameter
	~$ show vlan config

	Response
	Name    VID    Member    Mode
------  -----  --------  ------


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    Error:

	12
	Create VLAN 10 on SW-1
	SW-1
	18:56:42
	Pass

	Parameter
	~$ sudo config vlan add 10

	Response
	Success

	13
	Create VLAN 10 on SW-1
	SW-1
	18:56:48
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member    Mode
------  -----  --------  ------
Vlan10     10


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan10 10
not contain string:    Error:

	14
	Create VLAN 10 on SW-2
	SW-2
	18:56:53
	Pass

	Parameter
	~$ sudo config vlan add 10

	Response
	Success

	15
	Create VLAN 10 on SW-2
	SW-2
	18:56:59
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member    Mode
------  -----  --------  ------
Vlan10     10


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan10 10
not contain string:    Error:

	16
	Create VLAN 20 on SW-1
	SW-1
	18:57:04
	Pass

	Parameter
	~$ sudo config vlan add 20

	Response
	Success

	17
	Create VLAN 20 on SW-1
	SW-1
	18:57:10
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member    Mode
------  -----  --------  ------
Vlan10     10
Vlan20     20


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan20 20
not contain string:    Error:

	18
	Create VLAN 20 on SW-2
	SW-2
	18:57:16
	Pass

	Parameter
	~$ sudo config vlan add 20

	Response
	Success

	19
	Create VLAN 20 on SW-2
	SW-2
	18:57:21
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member    Mode
------  -----  --------  ------
Vlan10     10
Vlan20     20


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan20 20
not contain string:    Error:

	

	20
	Add VLAN 10 & VLAN 20 member on SW-1
	SW-1
	18:57:27
	Pass

	Parameter
	~$ sudo config vlan member add 10 Ethernet8

	Response
	Success

	21
	Add VLAN 10 & VLAN 20 member on SW-1
	SW-1
	18:57:32
	Pass

	Parameter
	~$ sudo config vlan member add 20 Ethernet8

	Response
	Success

	22
	Add VLAN 10 & VLAN 20 member on SW-1
	SW-1
	18:57:38
	Pass

	Parameter
	~$ sudo config vlan member add 10 -u Ethernet16

	Response
	Success

	23
	Add VLAN 10 & VLAN 20 member on SW-1
	SW-1
	18:57:44
	Pass

	Parameter
	~$ sudo config vlan member add 20 -u Ethernet20

	Response
	Success

	24
	Add VLAN 10 & VLAN 20 member on SW-1
	SW-1
	18:57:49
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member      Mode
------  -----  ----------  --------
Vlan10     10  Ethernet8   tagged
Vlan10     10  Ethernet16  untagged
Vlan20     20  Ethernet8   tagged
Vlan20     20  Ethernet20  untagged


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan10 10 Ethernet8 tagged
contain string:    Vlan10 10 Ethernet16 untagged
contain string:    Vlan20 20 Ethernet8 tagged
contain string:    Vlan20 20 Ethernet20 untagged
not contain string:    Error:

	25
	Add VLAN 10 & VLAN 20 member on SW-2
	SW-2
	18:57:55
	Pass

	Parameter
	~$ sudo config vlan member add 10 Ethernet4

	Response
	Success

	26
	Add VLAN 10 & VLAN 20 member on SW-2
	SW-2
	18:58:00
	Pass

	Parameter
	~$ sudo config vlan member add 20 Ethernet4

	Response
	Success

	27
	Add VLAN 10 & VLAN 20 member on SW-2
	SW-2
	18:58:06
	Pass

	Parameter
	~$ sudo config vlan member add 10 -u Ethernet12

	Response
	Success

	28
	Add VLAN 10 & VLAN 20 member on SW-2
	SW-2
	18:58:12
	Pass

	Parameter
	~$ sudo config vlan member add 20 -u Ethernet16

	Response
	Success

	29
	Add VLAN 10 & VLAN 20 member on SW-2
	SW-2
	18:58:17
	Pass

	Parameter
	~$ show vlan config

	Response
	Name      VID  Member      Mode
------  -----  ----------  --------
Vlan10     10  Ethernet4   tagged
Vlan10     10  Ethernet12  untagged
Vlan20     20  Ethernet4   tagged
Vlan20     20  Ethernet16  untagged


	Judgement
	Success

inter-conditional operator    :   and
contain string:    Vlan10 10 Ethernet4 tagged
contain string:    Vlan10 10 Ethernet12 untagged
contain string:    Vlan20 20 Ethernet4 tagged
contain string:    Vlan20 20 Ethernet16 untagged
not contain string:    Error:

	

	30
	Set Eth1 IPv4 Address on H-1
	H-1
	18:58:23
	Pass

	Parameter
	~$ sudo ip address add 10.0.100.10/24 dev Eth1

	Response
	Success

	31
	Set Eth1 IPv4 Address on H-1
	H-1
	18:58:23
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:01 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.10/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:201/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and
contain string:    inet 10.0.100.10/24
not contain string:    DOWN

	32
	Set Eth1 IPv4 Address on H-2
	H-2
	18:58:23
	Pass

	Parameter
	~$ sudo ip address add 10.0.100.11/24 dev Eth1

	Response
	Success

	33
	Set Eth1 IPv4 Address on H-2
	H-2
	18:58:23
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:02 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.11/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:202/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and
contain string:    inet 10.0.100.11/24
not contain string:    DOWN

	34
	Set Eth1 IPv4 Address on H-3
	H-3
	18:58:23
	Pass

	Parameter
	~$ sudo ip address add 10.0.200.10/24 dev Eth1

	Response
	Success

	35
	Set Eth1 IPv4 Address on H-3
	H-3
	18:58:23
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:03 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.12/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet 10.0.200.10/24 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:203/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and
contain string:    inet 10.0.200.10/24
not contain string:    DOWN

	36
	Set Eth1 IPv4 Address on H-4
	H-4
	18:58:23
	Pass

	Parameter
	~$ sudo ip address add 10.0.200.11/24 dev Eth1

	Response
	Success

	37
	Set Eth1 IPv4 Address on H-4
	H-4
	18:58:23
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:04 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.13/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet 10.0.200.11/24 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:204/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and
contain string:    inet 10.0.200.11/24
not contain string:    DOWN

	

	38
	Ping from H-1 to H-2
	H-1
	18:58:23
	Pass

	Parameter
	~$ ping -c 4 10.0.100.11

	Response
	PING 10.0.100.11 (10.0.100.11) 56(84) bytes of data.
64 bytes from 10.0.100.11: icmp_seq=1 ttl=64 time=4.67 ms
64 bytes from 10.0.100.11: icmp_seq=2 ttl=64 time=2.21 ms
64 bytes from 10.0.100.11: icmp_seq=3 ttl=64 time=2.18 ms
64 bytes from 10.0.100.11: icmp_seq=4 ttl=64 time=2.52 ms

--- 10.0.100.11 ping statistics ---
4 packets transmitted, 4 received, 0% packet loss, time 3005ms
rtt min/avg/max/mdev = 2.182/2.895/4.668/1.031 ms


	Judgement
	Success

inter-conditional operator    :   and
contain string:    64 bytes from 10.0.100.11
contain string:    4 packets transmitted, 4 received, 0% packet loss
not contain string:    From 10.0.100.10

	39
	Ping from H-1 to H-3
	H-1
	18:58:26
	Pass

	Parameter
	~$ ping -c 4 -I Eth1 10.0.200.10

	Response
	PING 10.0.200.10 (10.0.200.10) from 10.0.100.10 Eth1: 56(84) bytes of data.
From 10.0.100.10 icmp_seq=1 Destination Host Unreachable
From 10.0.100.10 icmp_seq=2 Destination Host Unreachable
From 10.0.100.10 icmp_seq=3 Destination Host Unreachable
From 10.0.100.10 icmp_seq=4 Destination Host Unreachable

--- 10.0.200.10 ping statistics ---
4 packets transmitted, 0 received, +4 errors, 100% packet loss, time 3063ms
pipe 3


	Judgement
	Success

inter-conditional operator    :   and
contain string:    From 10.0.100.10
contain string:    4 packets transmitted, 0 received, +4 errors, 100% packet loss
not contain string:    64 byte from 10.0.200.10

	

	40
	Delete Eth1 IPv4 Address on H-1
	H-1
	18:58:32
	Pass

	Parameter
	~$ sudo ip address del 10.0.100.10/24 dev Eth1

	Response
	Success

	41
	Delete Eth1 IPv4 Address on H-1
	H-1
	18:58:32
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:01 brd ff:ff:ff:ff:ff:ff
    inet6 fe80::5054:ff:fe10:201/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    DOWN
not contain string:    inet 10.0.100.10/24

	42
	Delete Eth1 IPv4 Address on H-2
	H-2
	18:58:32
	Pass

	Parameter
	~$ sudo ip address del 10.0.100.11/24 dev Eth1

	Response
	Success

	43
	Delete Eth1 IPv4 Address on H-2
	H-2
	18:58:32
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:02 brd ff:ff:ff:ff:ff:ff
    inet6 fe80::5054:ff:fe10:202/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    DOWN
not contain string:    inet 10.0.100.11/24

	44
	Delete Eth1 IPv4 Address on H-3
	H-3
	18:58:32
	Pass

	Parameter
	~$ sudo ip address del 10.0.200.10/24 dev Eth1

	Response
	Success

	45
	Delete Eth1 IPv4 Address on H-3
	H-3
	18:58:32
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:03 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.12/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:203/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    DOWN
not contain string:    inet 10.0.200.10/24

	46
	Delete Eth1 IPv4 Address on H-4
	H-4
	18:58:32
	Pass

	Parameter
	~$ sudo ip address del 10.0.200.11/24 dev Eth1

	Response
	Success

	47
	Delete Eth1 IPv4 Address on H-4
	H-4
	18:58:32
	Pass

	Parameter
	~$ ip address show Eth1

	Response
	3: Eth1: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc fq_codel state UP group default qlen 1000
    link/ether 52:54:00:10:02:04 brd ff:ff:ff:ff:ff:ff
    inet 10.0.100.13/24 brd 10.0.100.255 scope global Eth1
       valid_lft forever preferred_lft forever
    inet6 fe80::5054:ff:fe10:204/64 scope link 
       valid_lft forever preferred_lft forever


	Judgement
	Success

inter-conditional operator    :   and

not contain string:    DOWN
not contain string:    inet 10.0.200.11/24
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